**AM60K**

**BASIC MODEL**

For dishwashing room of hotel, restaurant, employee dinning  
- Two able washing cycle 60s/90s  
benefits - able switch or door cycle start switch, simple to use  
- Thermostop feature, ensure rinse temperature above 82℃ per washing cycle  
- Built-in rinse pump, provide equal pressure  
- Patented anti-clog nozzles, provide for the most extensive spray pattern  
- Touch pad and front mounted control, monitor temperatures on LED display  
- Light alerting when washing cycle over  
- L-form heavy wash tank design, exert wash pump performance furthest  
- Tank heater with temperature sensor, make sure of wash temperature above 55℃  
- Slope-shape wash chamber to prevent the cleaning-wares are polluted by dirt  
water-drop  
- Automatic filling water, and water level self-control, prevent dry heating  
- Booster tank with high quality heat preservation material, reduce heat loss  
- Self-flushing strainer and removable basket collect large food particles easily  
- Self-draining wash pump, heavy-duty and fosra nitation

**TECHNICAL DATA**

- wash capacity: 60/40 Racks/h  
- water consumption: 3L/rack  
- wash temperature: 55-65℃  
- rinse temperature: 82-90℃  
- voltage: 380V/50Hz/3N  
- total loading: 15kW/17kW  
- loading height: 440 mm  
- rack size: 500×500 mm  
- dimensions: 642×701×1440(H)mm  
- origin: China