**AM60K**

**BASIC MODEL**

For dishwashing room of hotel, restaurant, employee dinning
- Two able washing cycle 60s/90s
benefits - able switch or door cycle start switch, simple to use
- Thermostop feature, ensure rinse temperature above 82℃ per washing cycle
- Built-in rinse pump, provide equal pressure
- Patented anti-clog nozzles, provide for the most extensive spray pattern
- Touch pad and front mounted control, monitor temperatures on LED display
- Light alerting when washing cycle over
- L-form heavy wash tank design, exert wash pump performance furthest
- Tank heater with temperature sensor, make sure of wash temperature above 55℃
- Slope-shape wash chamber to prevent the cleaning-wares are polluted by dirt
water-drop
- Automatic filling water, and water level self-control, prevent dry heating
- Booster tank with high quality heat preservation material, reduce heat loss
- Self-flushing strainer and removable basket collect large food particles easily
- Self-draining wash pump, heavy-duty and fosra nitation

**TECHNICAL DATA**

- wash capacity: 60/40 Racks/h
- water consumption: 3L/rack
- wash temperature: 55-65℃
- rinse temperature: 82-90℃
- voltage: 380V/50Hz/3N
- total loading: 15kW/17kW
- loading height: 440 mm
- rack size: 500×500 mm
- dimensions: 642×701×1440(H)mm
- origin: China