

**BASIC MODEL**

Hood-type dishwasher for straight through or corner operation

* Nominal capacity up to 60 racks/h or 1,080 plates/h or 2,160 glasses/h
* 3 automatic cycles: short, standard, intensive
* Ready to install - completely equipped: fill / drain hose, electrical cable, detergent dispenser, rinse aid dispenser, rinse pump, drain pump, back-flow prevente
* 1 plate rack P-18-12
* 1 universal flat rack B-00-07
* 1 plastic cutlery rack CB8

**PRODUCT ADVANTAGES**

* **VISIOTRONIC control**: single button control with remaining time indicator together with text and graphic display
* **Exhaust energy storage**: the fully enclosed 4-sided hood keeps steam and energy inside the system: energy saving up to 3 kW/h, less humidity in the kitchen area and better hygienic conditions
* **CLIP-IN wash and rinse arms**: wash and rinse arms can be removed with one hand and without any tools
* **EASY-CLEAN concept**: blue markings in the machine help the operator to identify the components which require cleaning

## TECHNICAL DATA

|  |  |
| --- | --- |
| Flexible drain hose 2,000 mm | 20mm inner / 25mm outer diam.   |
|  Fresh water connection:  pressure hose 2,000 mm flow pressure necesassary waterflow | R 3/4" inside0.5 - 10 bar max 60°Csoftener models:0.8 - 10 bar5 l/min |
|  Power cord |  2,500 mm |
|  Hoses for detergent and rinse agent |  2,000 mm each |
|  Cycle times 1) | 60 sec.90 sec.180 sec. |
|  Water consumption |  2.5 l / rack |
|  Tank capacity |  23 l |
|  Tank heating |  2.5 kW interlocked |
|  Power supply |  400 / 50 / 3 / N |
|  Booster loading |  6.2 kW |
|  Total loading |  7.1 kW / 3 x 16 A |
|  Pump capacity |  0.7 kW / 350 l/min |
|  Loading height |  440 mm |
|  Noise level |  66 dB(A) |
|  Weight gross / net |  121 / 101 kg |

1) To reach set rinse temperatures even with cold water connection, the actual cycle-times extend accordingly.