

**BASIC MODEL**

Hood-type dishwasher for straight through or corner operation

* Nominal capacity up to 60 racks/h or 1,080 plates/h or 2,160 glasses/h
* 3 automatic cycles: short, standard, intensive
* Ready to install - completely equipped: fill / drain hose, electrical cable, detergent dispenser, rinse aid dispenser, rinse pump, drain pump, back-flow prevente
* 1 plate rack P-18-12
* 1 universal flat rack B-00-07
* 1 plastic cutlery rack CB8

**PRODUCT ADVANTAGES**

* **VISIOTRONIC control**: single button control with remaining time indicator together with text and graphic display
* **Exhaust energy storage**: the fully enclosed 4-sided hood keeps steam and energy inside the system: energy saving up to 3 kW/h, less humidity in the kitchen area and better hygienic conditions
* **CLIP-IN wash and rinse arms**: wash and rinse arms can be removed with one hand and without any tools
* **EASY-CLEAN concept**: blue markings in the machine help the operator to identify the components which require cleaning

## TECHNICAL DATA

|  |  |
| --- | --- |
| Flexible drain hose 2,000 mm | 20mm inner / 25mm outer diam. |
| Fresh water connection:   pressure hose 2,000 mm  flow pressure   necesassary waterflow | R 3/4" inside 0.5 - 10 bar max 60°C softener models: 0.8 - 10 bar 5 l/min |
| Power cord | 2,500 mm |
| Hoses for detergent and rinse agent | 2,000 mm each |
| Cycle times 1) | 60 sec. 90 sec. 180 sec. |
| Water consumption | 2.5 l / rack |
| Tank capacity | 23 l |
| Tank heating | 2.5 kW interlocked |
| Power supply | 400 / 50 / 3 / N |
| Booster loading | 6.2 kW |
| Total loading | 7.1 kW / 3 x 16 A |
| Pump capacity | 0.7 kW / 350 l/min |
| Loading height | 440 mm |
| Noise level | 66 dB(A) |
| Weight gross / net | 121 / 101 kg |

1) To reach set rinse temperatures even with cold water connection, the actual cycle-times extend accordingly.